{"text_format":"2","workbook":"xls","n_sheets":8,"sheets":["レベラーシャーライン","スリッターライン","成形ライン・成形機","圧延機　ｱﾝｺｲﾗｰ　ﾘｺｲﾗｰ　ｺｲﾙｶｰ","レベラー単体","ｼｬｰ　ﾍﾞﾝﾀﾞｰ　ﾌﾟﾚｽ　切断機","ｸﾚｰﾝ　ｺｲﾙﾘﾌﾀｰ","ｺﾝﾌﾟﾚｯｻｰ、他"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"レベラーシャーライン","index":0,"n_rows":28,"n_cols":3,"rows_kept":28,"cut":false,"hidden":false,"merged":[[2,1,2,2]],"flags":["formulas_cached_only"]}
["中　古　機　械　リ　ス　ト"]
[null,"(ﾚﾍﾞﾗｰ ｼﾔｰﾗｲﾝ)"]
[]
["在庫№","仕　　　　　　様","メーカー"]
["SK010","ｼｬｰﾗｲﾝ"]
[null,"  板厚:0.8-6.0mm 板幅:1600mm  ｺｲﾙ内径：φ508mm"]
[null,"欠品：ﾗﾌﾚﾍﾞﾗｰ､ﾌｨﾆｯｼｭﾚﾍﾞﾗｰ､ｼﾔｰ前ﾋﾟﾝﾁﾛｰﾙｻｲﾄﾞｶﾞｲﾄﾞ、油圧ﾕﾆｯﾄ、電気制御機器、操作盤"]
["SK035","ﾚﾍﾞﾗｰﾗｲﾝ                          ﾗｲﾝ方向：左→右"]
[null,"0.6-4.5mmx500-1350mm ｺｲﾙ内径:508,610,710mm,ｺｲﾙ重量:15Ton 切断長:3500mm","住倉工業"]
[null,"欠品：ｱﾝｺｲﾗｰ"]
["SK036","ｼｬｰﾗｲﾝ                            ﾗｲﾝ方向：左→右"]
[null," 0.5-3.2mmx500-1830mm ｺｲﾙ内径:508,610mm  ｺｲﾙ重量:20Ton 切断長:4000mm ","摂津工作所"]
[null,"欠品：仕上ﾚﾍﾞﾗｰ"]
[null,"厚物ｼｬｰﾗｲﾝ　　　　ﾗｲﾝ方向左→右"]
["SK047"," 1.2-6.0mmx500-1830mm ｺｲﾙ内径:508,610mm  ｺｲﾙ重量:25Ton 切断長:500-6100mm","住倉工業"]
[null,"欠品：無し"]
["SK050","狭幅ｼｬｰﾗｲﾝ　　　　ﾗｲﾝ方向左→右"]
[null," ｽﾄｯﾌﾟｶｯﾄ  WRφ80mmx250w4/5本 PRφ150x250mmx2段 ﾓｰﾀｰ7.5kwHC","八木製作所"]
[null,"欠品："]
["SK072","ﾌﾞﾗﾝｷﾝｸﾞﾗｲﾝ　　　　　　　　ﾗｲﾝ方向：左→右","1974年"]
[null,"ｱﾝｺｲﾗｰ面長:600mm ﾋﾟﾝﾁﾛｰﾙ:φ85×450L ﾚﾍﾞﾗｰ:φ85×450L,3本/4本 　ﾌﾟﾚｽ：無し","伊達機械"]
[null,"欠品："]
["SK135","3.2×1350 ｼﾔｰﾗｲﾝ   ﾗｲﾝ方向 右→左　ﾗｲﾝ速度：20～80m/min"]
[null," 板厚：0.4-3.2mm 板幅：500～1350mm ｺｲﾙ内径：φ508mm ｺｲﾙ重量：18Ton    ","住倉工業"]
[null,"欠品：無し、全部揃っている"]
["SK136","1.6×570 ｼﾔｰﾗｲﾝ   ﾗｲﾝ方向 右→左　ﾗｲﾝ速度：  m/min"]
[null," 板厚：1.6mm 板幅：570mm ｺｲﾙ内径：φ508mm ｺｲﾙ重量：  Ton    "]
[null,"欠品：無し、全部揃っている"]

{"sheet":"スリッターライン","index":1,"n_rows":23,"n_cols":3,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["中　古　機　械　リ　ス　ト"]
[null,"(ｽﾘｯﾀｰﾗｲﾝ)"]
[]
["在庫№","仕　　　　　　様","メーカー"]
["SK008","ｻｲﾄﾞﾄﾘｰﾏｰﾗｲﾝ"]
[null,"  板厚: 0.23-3.2mm  板幅: 508-1295mm ｺｲﾙ内径: 508/610mm ｺｲﾙ重量: 20Ton","ﾅｶﾔﾏ/川崎電機"]
[null,"欠品：ｽﾘｯﾀｰ部"]
[]
["SK040","ｽﾘｯﾀｰ本体"]
[null," ｱｰﾊﾞｰ:φ230mmｘ1460mmL 　"]
[null,"欠品：駆動装置、"]
["SK043","2.3×500ﾐﾆｽﾘｯﾀｰ                   ﾗｲﾝ方向：右→左  ｺｲﾙ重量：3.5Ton","1976年"]
[null," 0.4-2.3×500mm ｺｲﾙ内径300,508mm  ｱｰﾊﾞｰ径φ80mm ﾗｲﾝｽﾋﾟｰﾄﾞ60m/min ","小野機工所"]
[null,"欠品：ｱﾝｺｲﾗｰ､"]
["SK133","1.2×600mm  ｽﾘｯﾀｰﾗｲﾝ","1985年"]
[null," 板厚：0.2-1.2mm 板幅：30～600mm ｺｲﾙ内径：φ508mm ｺｲﾙ重量：3Ton    ","名古屋珪素鋼板"]
[null,"欠品：無し、全部揃っている"]
["SK143","0.4×1200 ｼｰﾄｽﾘｯﾀｰ(ｶﾞﾝｸﾞｽﾘｯﾀｰ)","1995年"]
[null,"板厚：0.15～0.4mm  板巾：450～1200mm  板長：450～1200mm","大阪製缶機械"]
[null,"欠品：無し、全部揃っている"]
["SK597","2.0x625mm ﾐﾆｽﾘｯﾀｰﾗｲﾝ"]
[null,"板厚：0.3-2.0mm  板巾：25～625mm ｺｲﾙ内径 : 508mm ｺｲﾙ重量 : 3.5Ton","協和工業"]
[null,"欠品：無し、全部揃っている"]

{"sheet":"成形ライン・成形機","index":2,"n_rows":74,"n_cols":3,"rows_kept":74,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["中　古　機　械　リ　ス　ト"]
[null,"(成形ﾗｲﾝ､成形機)"]
[]
["在庫№","仕　　　　　　様","メーカー"]
["SK009","1090W ﾌｫｰﾐﾝｸﾞﾗｲﾝ","1967年"]
[null,"  板厚: 0.5-1.6mm  板幅:MAX1090mm  ","冷間ﾛｰﾙ成形"]
[null,"欠品：電気制御機器、操作盤"]
["SK037","3m 切板 波付機 　板厚：0.27-0.6mm 板幅：1000mm 板長さ：3000mm 波型：小波","1965年"]
[null,"ﾄﾞﾗﾑ径：φ340mm ﾄﾞﾗﾑ面長：3140mm 電動機：11kw 4P","深田鉄工"]
[null,"欠品：駆動ｷﾞﾔ‐１部欠損有り"]
["SK052","C型鋼成形ﾗｲﾝ       ﾗｲﾝ方向右→左"]
[null," ﾀﾞｲｶｯﾄ ﾐﾙ:10段, ﾋﾟｯﾁ:330mm  軸径:φ55mmx400mm ﾓｰﾀｰ:AC30kw","八木製作所"]
[null,"欠品：ﾛｰﾙ金型"]
["SK053","C型鋼成形ﾗｲﾝ      ﾗｲﾝ方向左→右"]
[null," ｽﾄｯﾌﾟｶｯﾄ ﾐﾙ:12段, ﾋﾟｯﾁ:330mm  軸径:φ55mmx380mm ﾓｰﾀｰ:AC45kw ","八木製作所"]
[null,"欠品：ﾛｰﾙ金型"]
["SK055","破風及びメジ板成形ﾗｲﾝ      ﾗｲﾝ方向左→右     ﾓｰﾀｰ:AC45kw","1975年"]
[null," ﾐﾙ 1 :16段, ﾋﾟｯﾁ:350mm  軸径:φ40mm×350mm  ﾀﾞｳﾝｶｯﾄ"]
[null," ﾐﾙ 2 : 8段, ﾋﾟｯﾁ:500mm  軸径:φ50mm×300mm","東亜工機"]
[null,"欠品：ﾛｰﾙ金型"]
["SK056","PU型鋼成形ﾗｲﾝ      ﾗｲﾝ方向右→左","1975年"]
[null," ﾘﾐｯﾀｰｽﾄｯﾌﾟｶｯﾄ ﾐﾙ:6段, ﾋﾟｯﾁ:655mm  軸径:φ140mmx300mm ﾓｰﾀｰ:AC55kw","東亜工機"]
[null,"欠品：ﾛｰﾙ金型"]
["SK074","ﾌﾘｰｱﾝｸﾞﾙﾌｫｰﾐﾝｸﾞﾗｲﾝ   ﾗｲﾝ方向：左→右　電動機：22kw×220V×6P","1975年"]
[null," 板厚：1.4-2.3mm 板幅：60-130mm ﾐﾙ：10段 ﾋﾟｯﾁ:350mm　軸径：φ45mm×300mm","NAKATA"]
[null,"欠品：電気制御機器"]
["SK091","2.5m 切板 波付機"]
[null,"ﾄﾞﾗﾑ径：φ340mm ﾄﾞﾗﾑ面長：2580mm　波型：大波"]
[null,"欠品：駆動装置、操作盤"]
["SK094","ﾊﾟﾈﾙ成形ﾗｲﾝ      ﾗｲﾝ方向:左→右  ﾓｰﾀｰ:DC30kw　","1994年"]
[null," 成形ﾐﾙ :35段, 軸φ60×650mm ﾗｲﾝ速度：12m/min(成形のみ：50m/min) ","児島長"]
[null,"欠品：無し、全部揃っている"]
["SK106","P-400 切板成形機    ﾗｲﾝ速度：15m/min (機械ｻｲｽﾞ：1.12m×10m×1.2m、H)"]
[null," ﾐﾙ : 16段,  軸:φ75mm×950mm  ﾋﾟｯﾁ：590mm  電動機：5.5kw         ","協和成形機"]
[null,"欠品：成形機本体のみ、前後設備無し、成形ﾛｰﾙ組み込み済み"]
["SK107","P-450 切板成形機    ﾗｲﾝ速度：15m/min (機械ｻｲｽﾞ：1.13m×10m×1.4m、H)"]
[null," ﾐﾙ : 16段,  軸:φ75mm×950mm  ﾋﾟｯﾁ：610mm  電動機：3.7kw         ","協和成形機"]
[null,"欠品：成形機本体のみ、前後設備無し、成形ﾛｰﾙ組み込み済み"]
["SK108","P-500S 切板成形機    ﾗｲﾝ速度：15m/min (機械ｻｲｽﾞ：1.1m×7m×1.1m、H)","1996年"]
[null," ﾐﾙ : 12段,  軸:φ75mm×1000mm  ﾋﾟｯﾁ：570mm  電動機：3.7kw         ","協和成形機"]
[null,"欠品：成形機本体のみ、前後設備無し、成形ﾛｰﾙ組み込み済み"]
["SK109","P-500S 切板成形機    ﾗｲﾝ速度：15m/min (機械ｻｲｽﾞ：1.1m×7m×1.1m、H)"]
[null," ﾐﾙ : 12段,  軸:φ75mm×1000mm  ﾋﾟｯﾁ：570mm  電動機：3.7kw         ","協和成形機"]
[null,"欠品：成形機本体のみ、前後設備無し、成形ﾛｰﾙ組み込み済み"]
["SK110","P-500 切板成形機    ﾗｲﾝ速度：15m/min (機械ｻｲｽﾞ：1.3m×12m×1.3m、H)"]
[null," ﾐﾙ : 17段,  軸:φ75mm×1000mm  ﾋﾟｯﾁ：725mm  電動機：5.5kw         ","協和成形機"]
[null,"欠品：成形機本体のみ、前後設備無し、成形ﾛｰﾙ組み込み済み"]
["SK111","P-600 切板成形機    ﾗｲﾝ速度：15m/min (機械ｻｲｽﾞ：1.3m×11m×1.2m、H)"]
[null," ﾐﾙ : 20段,  軸:φ75mm×1150mm  ﾋﾟｯﾁ：515mm  電動機：5.5kw         ","協和成形機"]
[null,"欠品：成形機本体のみ、前後設備無し、成形ﾛｰﾙ組み込み済み"]
["SK112","BL-500 切板成形機    ﾗｲﾝ速度：15m/min (機械ｻｲｽﾞ：1.1m×14m×1.1m、H)"]
[null," ﾐﾙ : 27段,  軸:φ80mm×950mm  ﾋﾟｯﾁ：660mm 300mm 電動機：5.5kw         ","協和成形機"]
[null,"欠品：成形機本体のみ、前後設備無し、成形ﾛｰﾙ組み込み済み"]
["SK114","立平葺-300 切板成形機  ﾗｲﾝ速度：15m/min (機械ｻｲｽﾞ：0.7m×3m×0.9m、H)"]
[null," ﾐﾙ : 12段,  軸:φ50mm×600mm  ﾋﾟｯﾁ：220mm  電動機：3.7kw         ","清水機械"]
[null,"欠品：成形機本体のみ、前後設備無し、成形ﾛｰﾙ組み込み済み"]
["SK115","立平葺-400 切板成形機  ﾗｲﾝ速度：15m/min (機械ｻｲｽﾞ：0.7m×2m×0.9m、H)"]
[null," ﾐﾙ : 9段,  軸:φ35mm×600mm  ﾋﾟｯﾁ：200mm  電動機：1.5kw         ","清水機械"]
[null,"欠品：成形機本体のみ、前後設備無し、成形ﾛｰﾙ組み込み済み"]
["SK116","ｴﾊﾞﾙｰﾌ 1型成形機    ﾗｲﾝ速度：15m/min (機械ｻｲｽﾞ：0.5m×4m×0.8m、H)"]
[null," ﾐﾙ : 14段,  軸:φ35mm×450mm  ﾋﾟｯﾁ：240mm  電動機：1.5kw         ","清水機械"]
[null,"欠品：成形機本体のみ、前後設備無し、成形ﾛｰﾙ組み込み済み"]
["SK119","L21×21 ｱﾝｸﾞﾙ成形ﾗｲﾝ   ﾗｲﾝ方向：右→左　電動機：11kw×220V"]
[null," 板厚：1.6(2.3)mm  ﾐﾙ：7段 ﾋﾟｯﾁ:290-340mm　軸径：φ50mm"]
[null,"欠品：無し、全部揃っている"]
["SK123","C型鋼成形ﾗｲﾝ  ﾗｲﾝ方向：右→左　電動機：55kw×220V× P"]
[null," 板厚：2.3-3.2mm 板幅：500mm ﾐﾙ：14段 ﾋﾟｯﾁ:640mm　軸径：φ80mm×530mm"]
[null,"欠品：無し、全部揃っている"]
["SK145","JIS 小波成形機"]
[null," 波型：小波　ﾋﾟｯﾁ：32mm　高さ：9mm　働き幅：765mm"]
[null,"欠品：成形機本体のみ、前後設備無し、成形ﾛｰﾙ組み込み済み"]
["SK146","JIS 大波成形機"]
[null," 波型：大波　ﾋﾟｯﾁ：76.2mm　高さ：17mm　働き幅：720mm"]
[null,"欠品：成形機本体のみ、前後設備無し、成形ﾛｰﾙ組み込み済み"]

{"sheet":"圧延機　ｱﾝｺｲﾗｰ　ﾘｺｲﾗｰ　ｺｲﾙｶｰ","index":3,"n_rows":34,"n_cols":3,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["中　古　機　械　リ　ス　ト"]
[null,"(圧延機　ｱﾝｺｲﾗｰ ﾘｺｲﾗｰ ｺｲﾙｶｰ)"]
[]
["在庫№","仕　　　　　　様","メーカー"]
["SK038","ｱﾝｺｲﾗｰ                            ﾗｲﾝ方向：左→右  ｺｲﾙ重量：15Ton                       ","1967年"]
[null," ﾄﾞﾗﾑ径:φ508& 610mm(ｱﾀｯﾁﾒﾝﾄ付）面長:1600mm　ﾗｲﾝﾋｽﾋﾟｰﾄﾞ:80m/min  ","摂津工作所"]
[null,"欠品："]
["SK058","4巾 ｱﾝｺｲﾗｰ       ｺｲﾙｶｰ　ｽﾗｲﾄﾞﾍﾞｰｽ　押さえﾛｰﾙ 油圧装置付","1970年"]
[null," φ510mm×1350mmW, ｺｲﾙ重量：8Ton, ﾓｰﾀｰ:AC5.5kw 住友ｻｲｸﾛﾄﾞﾗｲﾌﾞ付","日立"]
[null,"欠品："]
["SK061","ﾘｺｲﾗｰ             4巾ﾘｺｲﾗｰ","1968年"]
[null," φ510mm×1470mmW  ｺｲﾙ重量：15T  ﾓｰﾀｰDC5.5kw","川崎電機"]
[null,"欠品："]
["SK062","ｱﾝｺｲﾗｰ","1972年"]
[null," ﾓｰﾀｰ AC5.5kw ｻｲｸﾛﾄﾞﾗｲﾌﾞ付","川崎電機"]
[null,"欠品："]
["SK064","ｱﾝｺｲﾗｰ","1968年"]
[null," φ250mm (φ610mm)×1400mmW ﾓｰﾀｰAC3.7kw","佐世保重工業"]
[null,"欠品："]
["SK067","ﾘｺｲﾗｰ             4巾ﾘｺｲﾗｰ","1982年"]
[null," φ508mm×1400mmW (φ610mm用は交換ﾄﾞﾗﾑ有り）","渡辺鉄工所"]
[null,"欠品："]
["SK104","ｺｲﾙｶｰ"]
[null,"荷台ｻｲｽﾞ：800mm×950mm　昇降：油圧"]
[null,"欠品："]
["SK105","ｺｲﾙｶｰ"]
[null,"荷台ｻｲｽﾞ：910mm×1500mm 昇降：油圧","攝津工作所"]
[null,"欠品："]
["SK117","ｱﾝｺｲﾗｰ     型式：ﾀﾞﾌﾞﾙｺｰﾝﾀｲﾌﾟ       (機械ｻｲｽﾞ：1.0m×2.1m×1.0m、H)"]
[null," ｺｲﾙ内径：φ508mm  ｺｲﾙ外形：φ1200mm ｺｲﾙ巾：1000mm ｺｲﾙ重量：1Ton"]
[null,"欠品："]
["SK142","635mm幅 ｺｰﾙﾄﾞﾚﾊﾞｰｽﾐﾙ            ﾗｲﾝ方向：右→左","1967年"]
[null,"板厚：0.2～4.2mm  板巾：350～635mm   ﾐﾙ電動機：DC220kw  ｺｲﾙ重量：6.5Ton","日立製作所"]
[null,"欠品：電気制御機器、MGｾｯﾄ、ﾍﾟｲｵﾌﾘｰﾙ､ｽﾘｰﾛｰﾙﾌｨｰﾀﾞｰ､配管類、配線類"]

{"sheet":"レベラー単体","index":4,"n_rows":24,"n_cols":3,"rows_kept":24,"cut":false,"hidden":false,"merged":[[2,1,2,2]],"flags":["formulas_cached_only"]}
["中　古　機　械　リ　ス　ト"]
[null,"(ﾚﾍﾞﾗｰ 単体)"]
[]
["在庫№","仕　　　　　　様","メーカー"]
["SK011","6Hi 1500W ﾃﾝｼｮﾝﾚﾍﾞﾗｰ　　　ﾗｲﾝ方向：左→右","1968年"]
[null," WR: φ50X1500 上12本/下11本､､中間:φ50X1500 上13本/下12本  ","IHI/東芝"]
[null,"BUR: φ100X65 上4列/下4列"]
[null,"欠品：　駆動ﾓｰﾀｰ　WR駆動ｽﾋﾟﾝﾄﾞﾙ　"]
["SK012","6Hi 1500W ﾃﾝｼｮﾝﾚﾍﾞﾗｰ     ﾗｲﾝ方向：右→左","1970年"]
[null," WR: 38X1500X17本､ 中間:32X1550X19本　BUR:上(82X10)本/下(82X11)本","日立"]
[null,"欠品：駆動ﾓｰﾀｰ  圧下ﾓｰﾀｰ　WR駆動ｽﾋﾟﾝﾄﾞﾙ"]
["SK013","4Hｲ 1450W ﾛｰﾗｰﾚﾍﾞﾗｰ     ﾗｲﾝ方向：左→右","1960年"]
[null," WR:80X1450X16本､ BUR: 80X286X54本（3列）　圧下ﾓｰﾀｰ：3.7kw×4P(2台）","日立"]
[null,"欠品：駆動ﾓｰﾀｰ　WR駆動ｽﾋﾟﾝﾄﾞﾙ 4本"]
["SK029","4Hi 3.2×1300 ﾚﾍﾞﾗｰ     ﾗｲﾝ方向：左→右","1967年"]
[null," WR：φ50×1400 上8本/下9本　BUR：3列　圧下ﾓｰﾀｰ：0.75kw×4P (2台）  ","新潟鉄工所"]
[null,"欠品：駆動ﾓｰﾀｰ　WR駆動ｽﾋﾟﾝﾄﾞﾙ 8本  上WR軸受け　WR 2本"]
["SK078","4H M&Tﾚﾍﾞﾗｰ   電動機：AC5.5kw×6P  440V     ﾗｲﾝ方向：左→右","1975年頃"]
[null,"WR：φ65mm×2000mm 10本/下11本　BUR：φ65×350mm×3列 上33本/下36本","鋼板造機工業"]
[null,"圧下ﾓｰﾀｰ：3.7kw×4P"]
[null,"欠品：駆動ﾓｰﾀｰ　WR駆動ｽﾋﾟﾝﾄﾞﾙ  　WR 2本"]
["SK086","4Hi×1500W ﾍﾋﾞｰﾚﾍﾞﾗｰ          ﾗｲﾝ方向：左→右","1964年"]
[null,"WR：φ80mm×1500mm　上7本/下8本  駆動電動機：DC55kw×220V 350/1300rpm","SUECO"]
[null,"欠品：BUR調整用ﾓｰﾀｰ(3台の内の1台破損）"]

{"sheet":"ｼｬｰ　ﾍﾞﾝﾀﾞｰ　ﾌﾟﾚｽ　切断機","index":5,"n_rows":26,"n_cols":3,"rows_kept":26,"cut":false,"hidden":false,"merged":[[1,1,1,2]],"flags":["formulas_cached_only"]}
["中　古　機　械　リ　ス　ト"]
[null,"(ｼﾔ- ﾍﾞﾝﾀﾞｰ ﾌﾟﾚｽ 切断機)"]
[]
["在庫№","仕　　　　　　様","メーカー"]
["SK017","3.0mm X 4000mmW ｷﾞｬｯﾌﾟｼｬｰ"]
[null,"  材料: ｽﾃﾝﾚｽ鋼板(抗張力:60kg/mm2) 刃長さ:4230mm ｽﾄﾛｰｸ数:60回/min","住友機械"]
["SK030","油圧式ｱｯﾌﾟｶｯﾄｼｬｰ"]
[null," ﾌﾞﾚｰﾄﾞ1400mmL","東研"]
["SK049","直線切断機","1994年"]
[null," 形式：F-2  電動機：22kw×4P×220V","藤井直線機"]
["SK057","ﾕﾆｶｯﾀｰ  （2台）","1974年"]
[null," UF-50   ﾎﾟﾝﾁﾝｸﾞ部加圧力：30Ton ｱﾝｸﾞﾙ部加圧力：50Ton  ｽﾄﾛｰｸ：40mm","藤村製作所"]
["SK059"," 2.5mm×4000mmW ｷﾞｬｯﾌﾟｼﾔｰ","1962年"]
[null," ｽﾄﾛｰｸ 60回/min　ﾓｰﾀｰ5.5kw","住友機械"]
["SK063","ｾﾐｵｰﾄｼﾔ－","1971年"]
[null,"3.2mm×1219mm 電動ﾊﾞｯｸｹﾞｰｼﾞ　ｶｯﾄ後ﾏｸﾞﾈｯﾄｻﾎﾟｰﾄ付","野間"]
["SK070","鋼管切断機      能力　ｿﾘｯﾄﾞ：φ10-60mm ﾊﾟｲﾌﾟ：φ10-90mm","1983年"]
[null,"型式：CM-400  刃物径：φ280mm ×2.5mmt 　　　　　　　 2台","AMADA"]
["SK071","鋼管切断機      能力　ｿﾘｯﾄﾞ：φ10-60mm ﾊﾟｲﾌﾟ：φ10-90mm","1982年"]
[null,"型式：KLN-2   刃物径：φ280mm ×2.5mmt　　　　　　　　","津根精機"]
["SK076","1.6×1600 ｱｯﾌﾟｶｯﾄｼﾔｰ 　ｸﾗﾝｸ式ｱｯﾌﾟｶｯﾄ (ｲﾝﾗｲﾝﾀｲﾌﾟ)"]
[null,"ﾌﾞﾚｰﾄﾞ長さ：1800mm 電動機：5.5kw×6P×440V","住倉工業"]
["SK138","4.5(6.0)×3000 ｼｬｰﾘﾝｸﾞ","1972年"]
[null,"油圧ﾀﾞｳﾝｶｯﾄｼﾔｰ","ｱﾏﾀﾞ"]
["SK140","4.5mm×4m ｼﾔｰﾘﾝｸﾞ    型式：ｱﾏﾀﾞＭ4045","1987年"]
[null,"板厚：4.5mm  板巾：4055mm  ｽﾄﾛｰｸ数：50SPM  電動機：11kw  機械重量：11Ton","ｱﾏﾀﾞ"]

{"sheet":"ｸﾚｰﾝ　ｺｲﾙﾘﾌﾀｰ","index":6,"n_rows":24,"n_cols":3,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["中　古　機　械　リ　ス　ト"]
[null,"(ｸﾚｰﾝ､ｺｲﾙﾘﾌﾀｰ)"]
[]
[]
[]
["在庫№","仕　　　　　　様","メーカー"]
["SK019","電動ｺｲﾙﾘﾌﾀｰ　　（２台）","1970年"]
[null,"  吊荷重: 31Ton  形式: 水平開閉式 開度: 1900mm  開閉速度:2m/min","石川島造船化工機"]
[null,"欠品：制御盤、ｹｰﾌﾞﾙﾘｰﾙ､電気品は整備が必要"]
["SK021","電動ｺｲﾙﾘﾌﾀｰ　　（６台）","1971年"]
[null,"  吊荷重: 18Ton  形式: 水平開閉式 開度: 1900mm  開閉速度:2m/min","石川島造船化工機"]
[null,"欠品：制御盤、ｹｰﾌﾞﾙﾘｰﾙ､電気品は整備が必要"]
["SK080","22.5Ton ｺｲﾙﾘﾌﾀｰ","1974年"]
[null,"吊荷重：22.5Ton  自重：1,8Ton  水平開閉式","石川島造船化工機"]
[null,"欠品：制御盤、ｹｰﾌﾞﾙﾘｰﾙ､電気品は整備が必要"]
["SK129","2.8Ton ｳｵｰﾙｸﾚｰﾝ","1993年"]
[null," 定格荷重：2.8Ton　横行範囲：3m","技研工業"]
[null,"欠品：無し"]
["SK137","2Tonｼﾞﾌﾞｸﾚｰﾝ      （２台）"]
[null," 吊荷重：2Ton  ｱｰﾑ長さ：3,500mm  ﾎｲｽﾄﾒｰｶｰ:三菱電機","三菱電機"]
[null,"欠品：無し"]
["SK144","25Ton ｺｲﾙﾘﾌﾀｰ"]
[null," ｸﾞﾗﾋﾞﾃｨｰﾀｲﾌﾟ"]
[null,"欠品：ｶﾞｲﾄﾞ部品１部欠損あり"]

{"sheet":"ｺﾝﾌﾟﾚｯｻｰ、他","index":7,"n_rows":21,"n_cols":3,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["中　古　機　械　リ　ス　ト"]
[null,"(ｺﾝﾌﾟﾚｯｻｰ､他）"]
[]
[]
[]
["在庫№","仕　　　　　　様","メーカー"]
["SK025","研磨ﾗｲﾝ","1992年"]
[null," 板厚:0.5-1.2mm 板幅:800-1600mm ｺｲﾙ重量: 10t ﾗｲﾝ方向 左→右","三晃Eng"]
[null,"欠品：研磨装置本体部分"]
["SK046","ﾄﾗﾊﾞｰｻｰ"]
[null," 2000mmwｘ4650mmL 車輪ｹﾞｰｼﾞ:1430mm ﾋﾟｯﾁ:2000mm 車輪径:φ600mm"]
["SK073","ｽﾎﾟｯﾄｸｰﾗｰ"]
[null,"型式：SR40YT 冷媒：ﾌﾛﾝ22 電力：1.5/1.9kw 3φ220V        9台","日立冷熱"]
["SK083","15kw ｴｱｰｺﾝﾌﾟﾚｯｻｰ"]
[null,"型式：SOD-1506D ｽｸﾘｭｳ  圧力：8.0kg/cm2  容量：2.5m3/min","ｱﾄﾗｽｺﾌﾟｺ岩田"]
["SK085","ﾊﾟｲﾗｰ"]
[null,"ｻｲｽﾞ：2050mm×2450mm","米盛鉄工所"]
["SK087","ﾍﾞﾙﾄｺﾝﾍﾞｱｰ"]
[null,"荷台ｻｲｽﾞ：2300mm×3500mm  ﾍﾞﾙﾄ幅：1250mm  電動機：AC 3.7kw×4P"]
["SK128","油圧ﾕﾆｯﾄ"]
[null," 作動油ﾀﾝｸ寸法：950mm×1500mm×600mmH  電動機：22kw×6P"]